# ID 50792

For circular area one linear and one circular block needed.
Description | A circular area consists of a linear block as starting point and a circular block as circular description. The second motion block after starting a definition of a circular area must be followed by a circular block as circle description. See also [PROG// Monitoring work and protection areas]

Example with error:

%cirlcular area

N10 #CONTROL AREA START [ID51 PROT CIRC MIN_EXCU…

N20 G01 X150 Y200 F10000

N30 G01 X150 Y200 F10000

N40 #CONTROL AREA END

N50 M30

Corrected example:

%cirlcular area

N10 #CONTROL AREA START [ID51 PROT CIRC MIN_EXCU…

N20 G01 X150 Y200 F10000 (start point)

N30 G02 G162 I70 J150

N40 #CONTROL AREA END

N50 M30

Response | Class | 6 | Movement stop.
Solution | Class | 6 | Check and modify the area definition in the NC program
Parameter | %1: | Identification number [-]
Area ID
%2: | Error value [-]
Intersection of polygon lines
Error type | 1, Error message from NC program.