# ID 20886

None of the programmed axes has axis mode C-axis.
Description | When face machining with the command #FACE, none of the two indicated axis is configured for the C-axis mode. The configuration take place in the corresponding axis parameter lists.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check the axes used in the command and check the axis mode P-AXIS-00015 in the corresponding axis list.
Error type | 1, Error message from NC program.