# ID 70211

Master axis for cross-compensation not present.
Description | The specified master axis for cross compensation does not exist. See also [FCT-C5// Section: Cross compensation]
Response | Class | 7 | Controlled stop of concerned axis
Solution | Class | 7 | Specify a valid logical axis number see P-COMP-00005
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis see P-AXIS-00016
%2: | Logical axis number [-]
Specified logical axis number of the master axis, which is not present. (see P-COMP-00005)
%3: | Drive type [-]
Drive type of concerned axis, see P-AXIS-00020
%4: | Block number [-]
Block number of the NC program, in which the error occurred
Error type | 2, Error message by data transfer from parameter list into control device.