# ID 21577

Invalid edge number in profile description.
Description | With active function tube profile machining #CYL[], an invalid number of edges is programmed.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and correct programming
Parameter | %1: | Current value [-]
Number of profile edges
%2: | Lower limit value
Minimum number of profile edges
%3: | Upper limit value
Maximum number of profile edges
Error type | 1, Error message from NC program.