# Maximum position offset (P-AXIS-00414)

P-AXIS-00414 | Maximum position offset
Description | The correction value of the axis that was calculated via distance control may not exceed this machine data item. An error message is issued if this value is exceeded. The correction value is limited.
Parameter | kenngr.distc.max_deviation
Data type | SGN32
Data range | 0 ≤ max_deviation < MAX(SGN32)
Axis types | T, R
Dimension | T: 0.1µm | R: 0.0001 °
Default value | 50000
drive types. | SERCOS, Profidrive, CANopen
Remarks |