# Number of records to be read in (P-STUP-00100)

P-STUP-00100 | Number of records to be read in
Description | This parameter specifies an upper limit for the number of parameter data records to be read in. It serves to allocate memory during controller start-up. An error is issued if this number is exceeded while reading in the records.
Parameter | vol_comp[i].max_records
Data type | SGN32
Data range | 0 … MAX(SGN32)
Dimension | ----
Default value | 0
Remarks |