# Settings for measurement

## Additional information

- Measurement type (P-CHAN-00057)
- Error reaction with measurement type 1 (P-CHAN-00176)
- Active delay with measurement signal (P-CHAN-00214)
- Error reaction with measurement type 7 (P-CHAN-00266)
- Automatic travel range limit (P-CHAN-00268)
- Active dynamic for measurement run (P-CHAN-00296)
- Including ball radius in PCS measurement value (P-CHAN-00311)
- Allow already actuated probes when starting a measurement run (P-CHAN-00312)
- Measurement path without motion path (P-CHAN-00313)
- Switch over between physical and clone axes during a measurement run (P-CHAN-00326)
- Axes, measurement values and offsets in CS (P-CHAN-00327)