# ID 110149

Minimum speed is greater than the maximum speed of homing.
Description | The slow homing speed for CNC controlled homing exceeds the fast homing velocity.
Response | Class | 1 | The slow homing velocity is limited to the fast homing velocity.
Solution | Class | 1 |
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [1µm/s or 0,001°/s]
P-AXIS-00218
%3: | Limit value [1µm/s or 0.001°/s]
P-AXIS-00219
%4: | Corrected value [1µm/s or 0,001°/s]
P-AXIS-00218
Error type | 2, Error message by data transfer from parameter list into control device.