# ID 110141

Incremental feed rate is greater than the maximum permissible feed rate.
Description | With manual mode in “continuous jog mode”, the parameter P-AXIS-00077 defines the continuous jog velocity. The specified value is greater than the permissible maximum value and is limited to this value.
Response | Class | 1 | Warning and correction of parameter.
Solution | Class | 1 | Check and correct the parameter P-AXIS-00077
Parameter | %1: | Logical axis number
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [1µm/s or 0.001°/s]
Current velocity P-AXIS-00077.
%3: | Upper limit value [1µm/s or 0.001°/s]
Maximum permissible velocity.
%4: | Corrected value [1µm/s or 0.001°/s]
Corrected velocity P-AXIS-00077.
%5: | Current value [-]
Array index of the incorrect entry
Error type | 2, Error message by data transfer from parameter list into control device.
[1µm/s or 0.001°/s]