# ID 70403

The configured bit mask is too big for the configured data type.
Description | The bit mask configured in P-AXIS-00429 is larger than the maximum value of the data type configured in P-AXIS-00399.
Response | Class | 7 | Error message output, evaluation of drive functions is aborted.
Solution | Class | 6 | P-AXIS-00429 value must be adjusted.
Parameter | %1: | Current value [-]
%2: | Current value [-]
Name of the configured drive function (P-AXIS-00396).
%3: | Error value [-]
Configured value of P-AXIS-00429
%4: | Current value [-]
Configured data type (P-AXIS-00399).
%5: | Error value [-]
Permissible maximum value of P-AXIS-00429
Error type | -