# ID 50917

Invalid parameter setting, r_max_equidist , p_admin->param.r_max_scale..
Description | When the ORBIT channel is activated, the parameters for the maximum scaling and equidistant radius are defined with the command #TRACK CHAN ON [EXTEND="DR channel number" MAX_SCALE=<val> MAX_EQUID=<val>]. The error is output when the value for the maximum scaling radius is less than 0 or the value for the maximum equidistant radius is less than the maximum scaling radius.
Response | Class | 4 | Movement stop.
Solution | Class | 7 | Check and correct the programming of the values for MAX_SCALE and MAX_EQUID in #TRACK CHAN ON [EXTEND="DR channel number" MAX_SCALE=<val> MAX_EQUID=<val>] in the ORBIT channel.
Parameter | %1: | Current value [0.1 10^-3 mm or ø]
Value for MAX_EQUID in #TRACK CHAN ON [EXTEND="DR channel number" MAX_SCALE=<val> MAX_EQUID=<val>].
%2: | Current value [0.1 10^-3 mm or ø]
Value for MAX_SCALE in #TRACK CHAN ON [EXTEND="DR channel number" MAX_SCALE=<val> MAX_EQUID=<val>].
%3 | Current value [0.1 10^-3 mm or ø]
Difference between MAX_EQUID and MAX_SCALE.
%4 | Limit value [0.1 10^-3 mm or ø]
Limit for difference.
Error type | 1, Error message from NC program.