# ID 50065

Remaining interpolation path greater than remaining braking distance.
Description | With the function Edge bending active, the residual path P-CHAN-00030 defined in channel parameter list is reduced after activation of measurement signal via the measuring probe. The braking distance at speed 0 required at this point must be smaller than the residual path.

Note: The axis parameters P-AXIS-00001, P-AXIS-00002 and P-AXIS-00011, P-AXIS-00012 influence the braking distance.

For more information on edge bending see [PROG// Section: Edge bending (G108)].

Response | Class | 1 | Movement stop.
Solution | Class | 1 | Either enlarge P-CHAN-00030, or reduce the programmed feedrate in the edge bending motion blocks, or if possible increase of axis acceleration.
Parameter | %1: | Current value[0.1 µm or 0.0001°]
Required braking distance to feed 0.
%2: | Expected value [0.1 µm or 0.0001°]
Residual path depending on P-CHAN-00030 .
%3: | Current value[0.1 µm or 0.0001°]
Path distance of measurement actual positions and target positions.
%4: | Current value [1µm/s or 0.001°/s]
%5: | Current value[0.1 µm or 0.0001°]
Error type | 1, Error message from NC program.