# ID 13226

Failure in programmed velocities (@P5, @P6).
Description | The measuring velocity is defined by the parameters @P5 and @P6. The multiple ID shows which parameter is defined incorrectly: 1. @P5 = 0 minimum measuring velocity equal to zero 2. @P5< 0 minimum measuring velocity is negative 3. @P6 = 0 maximum measuring velocity equal to zero

4. @P6 < 0 maximum measuring velocity is negative

5. @P5 >= @P6 minimum measuring velocity is greater than or equal to the maximum

Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check and correct the two parameters @P5 and @P6.
Error type | 1, Error message from the NC program