# Feedhold mode (P-AXIS-00540)

P-AXIS-00540 | Feedhold mode to select the active feedhold interface
Description | This parameter enables the selection of the effective feedhold interface(s) of independent axes.
Parameter | kenngr.indp_feedhold_mode
Data type | UNS16
Data range | 0: Feedhold from channel and axis interface (default). 1: Feedhold from axis interface
Axis types | T, R
Dimension | T: ---- | R: ----
Default value | 0
Drive types | ----
Remarks | The term independent axes covers all functions comprising single axis interpolators (INDP, SAI) except for manual mode. This does not affect the function of internal feedhold interfaces (e.g. CNC reset). For manual mode, the effect of feedhold control signals can be defined by the parameter P-AXIS-00529 .