# ID 21736

Axis commands exclude each other.
Description | A combination of mutually exclusive spindle-specific axis commands is programmed. For example, feedforward control and acceleration weighting are both programmed in one NC block: Wrong: N10 S[M03 S1000 G136=80 G130=60] :

N1000 M30

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and adjust syntax. Split the programming of weightings into 2 NC blocks.
Error type | 1, Error message from NC program.