# ID 110451

Modification of parameter p1043 requires restart of the control.
Description | Parameter P-AXIS-00317 cannot be changed while the CNC kernel is running. The new value is not adopted; the previous active value remains valid.
Response | Class | 1 | None.
Solution | Class | 1 | Reboot the controller after changing P-AXIS-00317.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [-]
Current value of P-AXIS-00317.
%3: | Corrected value [-]
Corrected (old) value of P-AXIS-00317.
Error type | 2, Error message on data transfer of parameter lists to controller.