# ID 70425

Timeout after deactivating the additional interface. Filter not within position window.
Description | To smooth command values, a PT2 filter can be activated in the position controller for the additive command value interface (see P-AXIS-00438). if the interface is disabled, the axis can run through the filter slightly. The CNC generates this warning message, if the axis is not in standstill within a certain amount of time.

See also:

[HLI// Section: External axis commanding] for CNC build < 2800

[HLI// Section: External axis commanding] for CNC build > 2800

Response | Class | 1 | Warning output
Solution | Class | 1 | Reduce time constant P-AXIS-00438 of PT2 filter
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Upper limit value [µs]
Elapsed time after the deactivation of the additive command value interface
%3: | Upper limit value [-]
Elapsed CNC cycles after the deactivation of the additive command value interface
%4: | Current value [0.1 µm or 0.0001°]
Position lag: Filter output - filter input
%5: | Current value[-]
Time constant P-AXIS-00438 of the used PT2 filter
Error type | 11, Error message from position controller.