# ID 14399

The specified machining depth is too low for the selected geometry data.
Description | The specified machining depth is too low to maintain the transferred chamfer depth (chamfer depth).
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Reduce the chamfer width or increase the machining depth.
Error type | 1, Error message from the NC program