# ID 120471

Oscillation movement outside SLS.
Description | The oscillation movement of oscillating axis exceeds software limit switches. For more information on oscillation movement, see [FCT-A8// Section: Description [PROG// Section: Oscillating axes].
Response | Class | 2 | Program execution stop.
Solution | Class | 6 | Check oscillation zero position and excursion, or oscillation reversal positions. Programming of oscillation movement inside software limits.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [0.1 10^-3 mm or ø]
Oscillation reversal position 1.
%3: | Current value [0.1 10^-3 mm or ø]
Oscillation reversal position 2.
%4: | Lower limit value [0.1 10^-3 mm or ø]
Negative software limit switch P-AXIS-00177
%5: | Upper limit value [0.1 10^-3 mm or ø]
Positive software limit switch P-AXIS-00178
Error type | 1, Error message from NC program.