# Advanced Lifting

This method is recommended.

Advantages of the time-based method.

- A greater lifting height can be achieved using Advanced Lifting.
- Greater collision protection
- Advanced Lifting has no negative impact on lifting height caused by changes in feed rate or path override.
- Conventional lifting may result in Z axis overload.

## Notice

Advanced Lifting cannot be used when the HCS slope is employed.

A further exception is the computing time if the aim is to achieve a shorter computing time for technical reasons.

## Additional information

- Advanced Lifting properties
- Parameterisation
- Special cases