# ID 70263

Homing method (homing_type) of master-/slave axis is different.
Description | The entry P-AXIS-00299 is assigned differently for the master and slave axes of a gantry configuration.
Response | Class | 1 | Error message output, correction of P-AXIS-00299 of the slave axis to the value of the master axis..
Solution | Class | 1 | P-AXIS-00299 have the same value assigned to master and slave axis.
Parameter | %1: | Logical axis number [-]
Logical axis number of the slave axis (see P-AXIS-00016).
%2: | Logical axis number [-]
Logical axis number of the master axis (see P-AXIS-00016)
%3: | Error value [-]
Entry P-AXIS-00299 of the slave axis.
%4: | Error value [-]
Entry P-AXIS-00299 of the master axis.
%5: | Corrected value [-]
Corrected entry P-AXIS-00299 of the slave axis.
Error type | -