# ID 50655

Not enough block path available for path edge band path.
Description | The “Block global edge bending” function (G108) checks whether the edge bending residual path can be reduced when deselected by G107. Depending on the channel parameter P-CHAN-00227 the preliminary check of the block path distance is suppressed. In this case, an insufficiently long block path distance was programmed before deselection by G107.

For more information on edge bending see [PROG// Section: Edge bending (G108)].

Response | Class | 4 | Movement stop. .
Solution | Class | 6 | Check programmed movement before G107
Error type | 1, Error message from NC program.