# ID 110061

Number of revolutions in the event of modulo errors is less than 0.
Description | The number of modulo revolutions P-AXIS-00125 is zero (nil). For an active modulo compensation P-AXIS-00120 the number must be greater than zero (nil).
Response | Class | 1 | Initialization of Modulo revolutions with default value.
Solution | Class | 1 | Correction of the value in the parameter list
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [-]
P-AXIS-00125
%3: | Limit value [-]
%4: | Corrected value [-]
P-AXIS-00125
Error type | 2, Error message by data transfer from parameter list into control device.