# ID 110691

Reference monitoring is not supported by this drive type.
Description | Reference monitoring (antr.reference_check.*) is not possible for this drive type.
Response | Class | 1 | Warning output, parameters are reset to their default values.
Solution | Class | 1 | --
Parameter | %1: | Logical axis number [-]
Logical axis number Axis parameters of the axis affected
Error type | 2, Error message by data transfer from parameter list into control device.