# ID 120482

For circular area a full circle without endpoint needed.
Description | A circular area consists of a linear block as starting point and a circular block as circular description. The second moment block after started a area definition should be circular for the circle description of the area.. See also [PROG// Monitoring work and protection areas]

Example with error:

%cirlcular area

N10 #CONTROL AREA BEGIN [ID51 PROT CIRC MIN_EXCU…

N20 G01 X150 Y200 F10000

N30 G03 G162 I50 J0 X250 Y200 F10000

N40 #CONTROL AREA END

N50 M30

Corrected example:

%cirlcular area

N10 #CONTROL AREA BEGIN [ID51 PROT CIRC MIN_EXCU…

N20 G01 X150 Y200 F10000 (start point)

N30 G03 G162 I70 J150

N40 #CONTROL AREA END

N50 M30

Response | Class | 2 | Abort NC program processing.
Solution | Class | 6 | Check and modify the area definition in the NC program.
Parameter | %1: | Identification number [-]
Area ID
%2: | Initial value [0.1 10^-3 mm or ø]
Startpoint for the circle description.
%3: | Final value [0.1 10^-3 mm or ø]
Targetpoint for the circle description.
Error type | 1, Error message from NC program.