# ID 14371

Spindle speed not defined.
Description | A valid spindle speed must be programmed and the spindle must be activated by M3/M4 before the cycle is called up.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Specify a valid spindle speed and activate the spindle before the cycle is called.
Error type | 1, error message from the NC program