# ID 110498

Acceleration monitoring: factor for warning greater than for error.
Description | Tolerance factor for excessive acceleration warning is set higher than for an error.
Response | Class | 1 | Value for warning is set to value for error. If acceleration limit is exceeded, no warning is generated before an error occurs
Solution | Class | 1 | Set smaller value.
Parameter | %1: | Logical axis number [-]
%2: | Current value [0.1%]
%3: | Limit value [0.1%]
%4: | Corrected value [0.1%]
Error type | 2, Error message on data transfer of parameter lists to controller.