# ID 110496

Position window of axis filter too small.
Description | The tolerance window P-AXIS-00351 specified for the axis filters was too small. The program waits for the position window to be reached provided the axis filters are active (| unfiltered command value – filtered command value| < P-AXIS-00351) at reset, axis position request or exact stop. The permissible tolerance window cannot be specified as too small due to the restricted computational accuracy.
Response | Class | 1 | Warning output, automatic correction of P-AXIS-00351.
Solution | Class | 1 | Correct value in parameter list.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Error value [0.1 µm or 0,0001°]
Incorrect value for position window P-AXIS-00351
%3: | Lower limit value [0.1 µm or 0,0001°]
Smallest permissible value for position window P-AXIS-00351
%4: | Corrected value [0.1 µm or 0.0001°]
Corrected value of P-AXIS-00351
Error type | 2, Error message by data transfer from parameter list into control device.