# Restore coupling after RESET (P-CHAN-00104)

P-CHAN-00104 | Restore coupling after reset (synchronous operation)
Description | An active axis coupling (synchronous operation) is deselected by NC reset. Set this parameter to 1 if the axis coupling is to be reactivated automatically in the following NC program.
Parameter | synchro_data.restore_coupling_after_reset
Data type | BOOLEAN
Data range | 0/1
Dimension | ----
Default value | 0
Remarks | This parameter may only be used if all axes participating in the coupling exist in the basic configuration of the NC channel.