# Assigned logical axis number (P-SECO-00042)

P-SECO-00042 | Assigned logical axis number
Description | Logical axis number of the axis which causes a movement of the new node point (P-SECO-00040). The type and method of the axis link is specified in the parameter P-SECO-00047.
Parameter | input_log_ax_nr
Data type | UNS16
Data range | 0 < P-SECO-00042 < MAX(UNS16)
Dimension | ----
Default value | 0
Remarks |

Example taken from list:

:

linkpoint[0].name X_ACHSE

linkpoint[0].mountpoint GROUND

linkpoint[0].input_log_ax_nr 1

linkpoint[0].cs_init.position[0] 0.000000

linkpoint[0].cs_init.position[1] 0.000000

linkpoint[0].cs_init.position[2] 0.000000

linkpoint[0].cs_init.orientation[0][0] 1.000000

linkpoint[0].cs_init.orientation[0][1] 0.000000

linkpoint[0].cs_init.orientation[0][2] 0.000000

linkpoint[0].cs_init.orientation[1][0] 0.000000

linkpoint[0].cs_init.orientation[1][1] 1.000000

linkpoint[0].cs_init.orientation[1][2] 0.000000

linkpoint[0].cs_init.orientation[2][0] 0.000000

linkpoint[0].cs_init.orientation[2][1] 0.000000

linkpoint[0].cs_init.orientation[2][2] 1.000000

linkpoint[0].trans_rot TRANS_X

linkpoint[0].visible 0

linkpoint[0].inverse 0

: