# ID 110551

Decreasing path parameter not allowed.
Description | When configuring distance dependent dynamic weighting, the path parameters (P-AXIS-00432) are not configured in ascending order.
Response | Class | 1 | Warning output, the dynamic weighting factors of the entry with the smaller path parameter are replaced by the dynamic weighting factors of the entry with the bigger path parameter.
Solution | Class | 1 | Sort the entries for the dynamic weighting factors in ascending order.
Parameter | %1: | Logical axis number [-]
%2: | Current value [0.1 10^-3 mm or ø]
%3: | Current value [0.1 10^-3 mm or ø]
%4: | Corrected value [0.1 10^-3 mm or ø]
Error type | 2, Error message by data transfer from parameter list into control device.