# ID 21201

Double programming of spindle feed forward control.
Description | Error message is output when programming the spindle feedforward control (G135, G136, G137). Either feedforward control commands are programmed which are mutually exclusive (G135,G137) or they occur several times [PROG//Section: Spindle feedforward control].
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC command. Remove redundant or exclusive commands.
Error type | 1, Error message from NC program.