# ID 110461

Number of configured user telegram elements exceeds limit.
Description | During the configuration of drive functions, the number of telegram elements (P-AXIS-00398) configured to be written in the cyclic process data exceeded the maximum limit See [FCT-A10// Section: Description]
Response | Class | 3 | Program execution stop.
Solution | Class | 6 | Adjust value of VAL in the NC-program.
Parameter | %1: | Logical axis number [-]
For logical axis number of concerned axis, see P-AXIS-00016
%2: | Current value [-]
Drive type (P-AXIS-00020).
%3: | Current value [-]
%4: | Limit value [-]
%5: | Current value [-]
Error type | -