# ID 20064

Face turning axis is used twice in processing plane.
Description | Only one axis, the first or the second main axis, can be used as face turning axis. In this case, however, both axes have the property of a facing axis (P-AXIS-00015).
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the axes parameter settings. Only one of the main axes may be facing axis P-AXIS-00015.
Parameter | %1: | Logical axis number [-]
Error type | -