# Parameters

The following parameters are required to call the cycle:

Cycle parameters | Description
@P4 | Measurement path in X axis - Only positive value permitted
@P5 | Measurement path in Y axis - Only positive value permitted
@P6 | Measurement path in Z axis - Only positive value permitted
@P9 (optional) | Shift the measuring point along the X axis
@P10 (optional) | Shift the measuring point along the Y axis
@P11 (optional) | Shift the measuring point along the Z axis
@P17 | Pre-position in X
@P18 | Pre-position in Y
@P19 | Pre-position in Z
@P39 | Select the required CS to be written. Value range: 1-10
@P41 | Pre-position in X2
@P42 | Pre-position in X3
@P43 | Pre-position in Y2
@P44 | Pre-position in Y3
@P49 (optional) | Retraction height after measurement Default value = position after last measurement