# ID 20155

Double programmed M function for spindles.
Description | A spindle M function (M3/M4/M5/M19) in the NC block is programmed multiple times in spindle-specific syntax. Example: Wrong: N10 G00 X0 Y0 Z0 N20 X10 S[M3 S1000 M4]

:

N1000 M30

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the programming of the M functions in the NC block. Remove surplus spindle-specific M function.
Parameter | %1: | Error value [-]
Number of the double programmed spindle M function
Error type | 1, Error message from NC program.