# Homing without cam (P-AXIS-00156)

P-AXIS-00156 | Homing without cam
Description | A changeover of homing strategy can be carried out so that homing is done without cam (e.g. only with zero pulse), i.e. without reverting. In this case the parameter P-AXIS-00156 should be set to TRUE.
Parameter | kenngr.ref_ohne_nocken
Data type | BOOLEAN
Data range | 0/1
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 0
drive types. | Conventional, Terminal, Lightbus, Profidrive
Remarks | To be assigned for analogue spindles only. If P-AXIS-00156 is assigned with 1 (TRUE), then it is imperative that P-AXIS-00157 is assigned with 1 (TRUE).