# Parameters

## Required input parameters

Input parameters | Description
@P65 | Type 0 = length measurement 1 = radius measurement 2 = length and radius measurement
@P66 | Measurement offset in Z for lateral measurements [mm, inch] Only positive values are permissible.

## Optional input parameters

Input parameters | Description
@P13 | Clearance for lateral measurements [mm, inch] Default value = current tool diameter (V.G.WZ_AKT.R)
@P23 | Precision measurement repetitions Default value = 1
@P33 | Crossover range during measurement process [mm, inch] Default value = current tool diameter (V.G.WZ_AKT.R)
@P37 | Permissible tolerance of measuring point scatter. Default value = 1/100 * current tool diameter (0.01*V.G.WZ_AKT.R) If the difference of the measured values exceeds this tolerance, an error is output.
@P64 | Mode 0 = push (default value) 1 = pull
@P67 | Lateral offset for length measurements [mm, inch] Only positive values are permissible. The value should stand at 0 for pointed tools, small tools and spherical tools. Default value = 0

It is recommended to use the Syntax check.to verify whether the input parameters are correctly assigned.