# ID 60242

Command acceleration while synchronized in camming or gearing exceeded.
Description | The permissible command acceleration P-AXIS-00304 during camming or gearing was exceeded.
Response | Class | 6 | Stopping the axis, and aborting the NC program.
Solution | Class | 6 | Adapt command acceleration.
Parameter | %1: |
%2: | Current value [mm/s^2 bzw. °/s^2]
Current value of the commanded acceleration.
%3: | Limit value [mm/s^2 bzw. °/s^2]
Limit value of command acceleration P-AXIS-00304.
Error type | -