# ID 110236

Leadscrew error compensation activated without compensation value list.
Description | The CNC detects an inconsistent parameterisation regarding leadscrew error compensation. In an axis configuration list, the leadscrew error compensation was activated by the parameter P-AXIS-00175. The CNC now expects the information regarding the path and the name by which a corresponding compensation value list can be found. To do this, the data in parameters P-STUP-00016, P-STUP-00017, P-STUP-00036 must be parameterised correctly in start-up list.

The parameters P-COMP-00001 and P-COMP-00020 must also be entered correctly for leadscrew error compensation in the appropriate compensation value list.

Response | Class | 1 | CNC disables leadscrew error compensation.
Solution | Class | 7 | Check the parameters P-STUP-00016 P-STUP-00017 P-STUP-00036 P-COMP-00001
P-COMP-00020 for data consistency.

If leadscrew error compensation is not required, set the parameter P-AXIS-00175 to the value 0.

Parameter | %1: | Logical axis number [-]
Parameter P-AXIS-00016 from an axis configuration list where the leadscrew error compensation was activated by P-AXIS-00175.
Error type | 2, Error message on data transfer of parameter lists to controller.