# ID 50262

During measuring virtual and other axes must not be mixed.
Description | When using measuring function G100, virtual axes and axes of another drive type (P-AXIS-00020) are mixed in measurement axes. This is not permitted. For more information on the G100 measuring function, see [PROG// Section: Measuring functions] [FCT-C4].
Response | Class | 4 | Movement stop.
Solution | Class | 6 | For the drive type (P-AXIS-00020), use either only virtual axes or no virtual axes for the axes involved in the measurement run
Parameter | %1: | Current value [-]
Number of virtual measurement axes in measurement axis group.
%2: | Current value [-]
Programmed axes of measurement axis group.
Error type | 1, Error message from NC program.