# ID 110348

Terminal KL2521 can not be used for probing.
Description | A terminal of the KL2521 type cannot be used for measuring since it has no external latch input. The measurement function is disabled for this axis (see P-AXIS-00118).
Response | Class | 1 | Correction of parameter P-AXIS-00118
Solution | Class | 1 | Correct parameter P-AXIS-00118 or use other terminal type
Parameter | %1: | Logical axis number [-]
For logical axis number of concerned axis, see P-AXIS-00016
%2: | Current value [-]
Specified value of parameter P-AXIS-00118
%3: | Corrected value [-]
Corrected value for parameter P-AXIS-00118
Error type | 2, Error message by data transfer from parameter list into control device.