# Inverting 'Ready for Power' signal (P-AXIS-00710)

P-AXIS-00710 | Inverting 'Ready for Power' signal
Description | This parameter inverts the result of the calculation of the 'Ready for Power' signal.
Parameter | antr.add_ready_for_operation.inverted
Data type | BOOLEAN
Data range | 0/1
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 0
Drive types | Simulation, SERCOS, Profidrive, CANopen, Terminal
Remarks |