# Logical axis number of second adaptation axis (P-COMP-00081)

P-COMP-00081 | Logical axis number of the second adaptation axis
Description | This parameter defines the logical axis number of the second adaptation axis. The position of the adaptation axis influences compensation in Mode 3 (P-COMP-00082).
Parameter | kw.crosstalk.master_pos2_ax_nr
Data type | UNS16
Data range | 0 < P-COMP-00081 < MAX(UNS16)
Axis types | T
Dimension | T: ---- | R, S: -
Default value | 0
Remarks | Parameter available as of V3.1.3081.2 and V3.1.3108.4