# Logging mode (P-STUP-00167)

P-STUP-00167 | Logging mode of error output
Description | This parameter controls the output and scope of the error output.
Parameter | error_protocol_mode
Data type | STRING
Data range | Flag | Meaning
FILTER_OFF | No filters are evaluated
VERBOSE | Extended internal diagnostics
WITHOUT_ERROR_MANAGER | Direct output without error management
PRINT | Execute print output
LOG | Log output to log file
REPORT | Log output to log file
SEND_TO_PLC_NONE | Suppress output to the PLC
PRINT_EXTENDED | Extended print output
LOG_EXTENDED | Extended log output
REPORT_EXTENDED | Extended application-specific output
PRINT_NO_WARNINGS | Warnings are suppressed in the print output
LOG_NO_WARNINGS | Warnings are suppressed in the log output
REPORT_NO_WARNINGS | Warnings are suppressed in the report output
SEND_TO_PLC_NO_WARNINGS | Suppress warnings to PLC
STARTUP_NO_WARNINGS | Suppress warnings during controller start-up
NO_WARNINGS | Suppress all warnings
TC3_EVENT_LOGGER | Output to TC3 Event Logger
TC3_EVENT_LOGGER_CONFIRMED | Output to TC3 Event Logger, automatic confirmation (state confirmed) on deletion of error message
TC3_EVENT_LOGGER_NO_CONFIRMATION | Output to TC3 Event Logger without confirmation request
Dimension | ----
Default value | LOG | PRINT | REPORT
Remarks | Note: For example, to suppress warnings in the print output, the entire mode must be set accordingly. error_protocol_mode LOG | PRINT | REPORT | PRINT_NO_WARNINGS

## Notice

This parameter is provided with reduced scope in the Version V2.2810.xx. The following setting can be made:
error_protocol_mode NO_WARNINGS

Therefore, only warnings can be suppressed.