# Description of channel parameters

P-CHAN-00014 | Implicit execution of D word with T
Description | If a T command is programmed, the D command is implicitly executed with the same number as the T command. This mechanism can be selected both for a list-based internal and for an external tool management. This parameter has no effect on the programming of #TOOL PREP (corresponds to the T command). Afterwards, a #TOOL DATA must always be programmed.
Parameter | einrechnen_mit_t
Data type | BOOLEAN
Data range | 0/1
Dimension | ----
Default value | 0
Remarks | Parameterisation example: The parameter 'einrechnen_mit_t' is assigned the value 1. The programming of 'T80' then corresponds to the programming command 'T80 D80'. einrechnen_mit_t 1

P-CHAN-00016 | Tool data is requested from an external tool management
Description | If the system works with external tool management (e.g. integrated in PLC), this parameter is set to 1.
Parameter | ext_wzv_vorhanden
Data type | BOOLEAN
Data range | 0/1
Dimension | ----
Default value | 0
Remarks | Parameterisation example: The system works with an external tool management. ext_wzv_vorhanden 1

P-CHAN-00076 | Send tool life data to external tool management
Description | If an external tool management system is used, only tool data are requested from it by default. This parameter must also be set to send the tool life data of a tool determined in the NC kernel to the external tool management.
Parameter | tool_life_to_wzv
Data type | BOOLEAN
Data range | 0/1
Dimension | ----
Default value | 0
Remarks |

P-CHAN-00087 | Information of the external tool management in case of a T function
Description | Programming a T function generates a message which is sent to the external tool management to prepare the magazine for a tool change. Assignment is only executed if an external tool management is used ((P-CHAN-00016).
Parameter | t_info_to_wzv
Data type | BOOLEAN
Data range | 0/1
Dimension | ----
Default value | 0
Remarks | Parameterisation example: If a T function is programmed, the external tool management prepares a tool change. t_info_to_wzv 1

P-CHAN-00106 | Enabling motion blocks during T selection
Description | By setting the parameter to 1, all motion blocks up to the T word are executed. This is an implicit '#FLUSH CONTINUE’ initiated by the T word[PROG// Flushing NC channel]. Assignment only makes sense if an external tool management is used (P-CHAN-00016).
Parameter | t_with_implicit_flush
Data type | BOOLEAN
Data range | 0/1
Dimension | ----
Default value | 0
Remarks |

P-CHAN-00255 | Tool life data recording for rapid traverse motions
Description | With tool life data recording, no rapid traverse motions G00 are recorded by default. This parameter achieves that rapid traverse motions are also considered for tool life data recording.
Parameter | tool_life_capture_all_movements
Data type | BOOLEAN
Data range | 0: Rapid traverse motions G00 are not included in tool life data recording (default). 1: Rapid traverse motions G00 are also included in tool life data recording.
Dimension | ----
Default value | 0
Remarks |

P-CHAN-00243 | Suppress output of tool life parameters 0
Description | When parameter P-CHAN-00076 is set, the tool life data is sent to the external tool management on every tool change, even if this is zero. This parameter can be set if no tool life data is sent in the event that service distance and service life = zero .
Parameter | tool_life_to_wzv_suppress_zero
Data type | BOOLEAN
Data range | 0/1
Dimension | ----
Default value | 0
Remarks | This parameter is available as of CNC Build V2.11.2802.00 and higher.