# Defining logging levels

Bit 31 to Bit 16 for cross-BF log level classes | Description
0x00010000 BF_LOG_STD | Default BF events
0x00020000 BF_LOG_UPLOAD | #COLL/SCENE RESTORE
0x40000000 BF_LOG_HIGH | High priority events
0x80000000 BF_LOG_RESET | Events at BF reset
0xFFFFffff BF_LOG_ALL | All BF log entries are logged.

Bit 15 to Bit 0 for BF-specific log level classes | Description
0x00000001 BAHN_LOG_STD | Default Interpolator
0x00000002 BAHN_LOG_DDTG_ | Events at “Delete distance to go”
0x00000004 BAHN_LOG_FBC_ | Forward/backward motion
0x00000008 BAHN_LOG_BS_ | Block search

0x00000001 BAVO_LOG_STD | Default Bavo

0x00000001 DEC_LOG_STD | Default decoder
0x00000002 DEC_LOG_EXAMPLE_ | ---
0x00000004 DEC_LOG_VI | Interchannel variables

0x00000001 AXV_LOG_STD | Default axis exchange

0x00000001 LR_LOG_STD | Default position controller
0x00000002 LR_LOG_ALNK | Axis link from IPO to LR during channel output
0x00000004 LR_LOG_BODE_PLOT | Bode plot logging