# ID 21316

Tangential selection or deselection during active inner corner selection not allowed.
Description | When the inner corner selection of tool radius compensation (TRC) is active, the tangential selection or deselection with G05 is not permissible. The command G05 used is ignored. Example: Wrong: N10 G238 :

N100 G41 G05

N110 G01 X100 F1000

:

N1000 M30

Correct:

N10 G238

:

N100 G41

N110 G01 X100 F1000

:

N1000 M30

Response | Class | 1 | Continue NC program processing.
Solution | Class | 1 | Check and modify the NC program. Remove G05.
Parameter | %1: | Current value [-]
G function used
Error type | -