# ID 20577

No face turning axis configured for tool tip radius compensation.
Description | When the tool offsets are accepted with active tool tip radius compensation (SRK) for turning tools, it is detected that neither of the plane axes is configured as face turning axis P-AXIS-00015.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | For lathes in the axis parameter list, one of the plane axes (first or second main axis) must be configured as face turning axis P-AXIS-00015.
Parameter | %1: | Current value [-]
Axis mode of the axis
%2: | Expected value [-]
Number of the "face turning axis"
%3: | Logical axis number [-]
%4: | Logical axis number[-]
Error type | 1, Error message from NC program.