# ID 110412

Coefficient (gradient) of temperature compensation exceeds permissible value range.
Description | The compensation values of temperature compensation are approximated by a linear straight line. The pitch of the straight line is specified in parameter P-AXIS-00274 as a function of the temperature. However, the current value specified in the axis parameters list is outside the permissible value range.

See FCT-C5// Section: Temperature compensation

Response | Class | 1 | Warning, automatic correction of parameter P-AXIS-00274 to maximum or minimum permissible value.
Solution | Class | 1 | Correct the value of parameter P-AXIS-00274 in the axis parameter list.
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis (see P-AXIS-00016)
%2: | Error value [-]
Incorrect value for P-AXIS-00274
%3: | Limit value [-]
Largest allowed value for gradient pitch P-AXIS-00274
%4: | Limit value [-]
Smallest permissible value for gradient pitch P-AXIS-00274
%5: | Corrected value [-]
Corrected value for parameter P-AXIS-00274
Error type | -